**Axessor CIT - Electronic Safe Lock 82705**

The One Time Combination lock Axessor CIT is characterized by its Interactive Code System (ICS).

In ICS Mode the user registers at the lock with his personal ID. The ICS ensures on site presence and generates a temporary, person-related and situational specific One Time Question. Only after telephonic forwarding of this question to the dispatch centre and verification of the data, the user gets a One Time Code to open the lock from the dispatch centre. Every event is recorded to guarantee the maximum transparency.

EN 1300 B

VdS Class 2

UL Type 1

ECB●S

[**Features**](https://www.dormakaba.com/gb-en/solutions/products/safe-locks/axessor/axessor-cit-267876#features)

Approvals/Certificates

EN 1300 B, VdS Class 2, UL Type 1, ECB●S

VdS bolt switch for alarm systems class C

Codes (bank mode)

1 Master

4 Managers

36 Users

1 Courier

Audit

> 10.000 events

Power Supply

3 x 1.5 volt Alkaline batteries LR6/AA (included in delivery)

Input Unit

Metal housing in black

Silicon key pad, green navigation keys

LC display and buzzer

Integrated battery compartment

Lock Unit

Motor bolt, 5 N moving force in both directions

Adaptable bolt function: dead bolt or spring bolt (non-VdS) setting

Bolt with 2xM4 threads

Lock mounting set, incl. 3xM6 screws

e-Box

Networkmodul

5 x Outouts potential-free

5 x Inputs contact-controlled

2 x Axessor-Bus

1 x LAN

1 x external power supply

[Technical data](https://www.dormakaba.com/gb-en/solutions/products/safe-locks/axessor/axessor-cit-267876#technicalData)

Electronic combination lock

Axessor CIT

Input Units

Metal, black

Software

Activation software AS280-INSW (ICS/OTC/DM activation)

Included in delivery: USB connection cable, USB dongle

Programming software AS284-USBW (lock settings)

Included in delivery: USB connection cable, USB dongle (1x) to configure and parametrize locks for "stand alone" applications

Programming software AS284-NETW (lock settings)

Included in delivery: USB connection cable, USB dongle (4x) to configure and parametrize locks for network applications

Server Management Software AS 274

(Manage more than 100 locks and users)

Includes: 1 APHI Ethernet RJ45

Accessories

Dongle AS284-OW Operator

USB dongle for programming software AS284-USBW & AS284-NETW

Dongle AS284-AW Administrator

USB dongle for programming software AS284-NETW

[Functionality](https://www.dormakaba.com/gb-en/solutions/products/safe-locks/axessor/axessor-cit-267876#functionality)

Code Functions

One time combination with close code, incl. battery status and lock/door activity feedback

Temporary code validity

Switchable mode (one time combination and/or bank mode)

Wrong try lockout after 4 false codes

Duress code (silent alarm)

Single mode (1 x 6 digits)

Dual mode (2 x 6 digits)

Shelve function

Time Lock Functions

Time delay

Duress time delay

Opening window

time lock periods (bank mode)

Non-return time delay

Automatic DLST (summer/winter time) changeover

[Applications](https://www.dormakaba.com/gb-en/solutions/products/safe-locks/axessor/axessor-cit-267876#applications)

AS284-NETW Programming Software

Use the AS284-NETW software to configure and parametrize Axessor Series products like Axessor USB (stand alone only), Axessor IP and Axessor CIT.

In Axessor IP or Axessor CIT systems software AS284-NETW can be used for remote administration or networked operation in general (by using eBox).

Changes to previous version:

AS284-W version 4.0.0.63

Support for multiple AS284-W instances in virtualized environments

AS284-W version 4.0.0.61

Based on .Net 4.5 instead of 4.0

Preparation for audit viewer dongle

Preparation for SDK dongles

Several bug fixes

AS284-USBW Programming Software

Use the AS284-USBW software to configure and parametrize Axessor Series products like Axessor USB, Axessor IP and Axessor CIT.

This software is for stand alone purposes only (no networking functionality).

Changes to previous version:

AS284-W version 4.0.0.63

Support for multiple AS284-W instances in virtualized environments

AS284-W version 4.0.0.61

Based on .Net 4.5 instead of 4.0

Preparation for audit viewer dongle

Preparation for SDK dongles

Several bug fixes

AS280-INSW Installation/Activation Software

Use software AS280-INSW to install network locks (Axessor IP/CIT with eBox) and to activate one time combination mode (Axessor CIT only).

You need to be registered dormakaba SafeLocks to download this software. Please contact dormakaba SafeLocks Support sl-techsupport.ch@kaba.com.

Axessor CIT - Elektronik Güvenli Kilit 82705

Tek Kullanımlık Şifreli kilit Axessor CIT, İnteraktif Kod Sistemi (ICS) ile karakterize edilir.

ICS Modunda kullanıcı kilide kişisel kimliğiyle kaydolur. ICS, sahada bulunmasını sağlar ve geçici, kişiyle ilgili ve duruma özgü bir tek seferlik soru oluşturur. Ancak tek seferlik sorunun dağıtım merkezine telefonla yönlendirilmesinden ve verilerin doğrulanmasından sonra, kullanıcı kilidi dağıtım merkezinden bir açma kodu alır. Maksimum şeffaflığı garanti etmek için yapılan her işlemin kaydı tutulur.

* EN 1300 B
* VdS Sınıf 2
* UL Tip 1
* ECB ● S

**Özellikleri**

**Onaylar / Sertifikalar**

* EN 1300 B, VdS Sınıf 2, UL Tip 1, ECB ● S
* C sınıfı alarm sistemleri için VdS cıvata anahtarı

**Kodlar (banka modu)**

* 1 Usta
* 4 Yöneticiler
* 36 Kullanıcı
* 1 Kurye

**Denetim**

* 10.000 etkinlik

**Güç kaynağı**

* 3 x 1.5 volt Alkalin piller LR6 / AA (teslimata dahildir)

**Giriş ünitesi**

* Siyah metal gövde
* Silikon tuş takımı, yeşil gezinme tuşları
* LC ekran ve zil
* Entegre pil bölmesi

**Kilitleme Ünitesi**

* Motor cıvatası, her iki yönde 5 N hareket kuvveti
* Uyarlanabilir cıvata fonksiyonu: ölü cıvata veya yaylı cıvata (VdS olmayan) ayarı
* 2xM4 dişli cıvata
* Kilit montaj seti, dahil. 3xM6 vidalar

**E-Box**

* Networkmodul
* 5 x Kesintisiz
* 5 x Giriş kontrollü
* 2 x Axessor-Otobüs
* 1 x LAN
* 1 x harici güç kaynağı

**Teknik veri**

**Elektronik şifreli kilit**

* Axessor CIT

**Giriş Birimleri**

* Metal, siyah

**Yazılım**

**Aktivasyon yazılımı AS280-INSW (ICS / OTC / DM aktivasyonu)**

* Teslimat kapsamı: USB bağlantı kablosu

**Programlama yazılımı AS284-USBW (kilit ayarları)**

* Teslimat kapsamı: USB bağlantısı kablosu, "bağımsız" uygulamalar için kilitleri yapılandırmak ve parametreleri ayarlamak için USB donanım kilidi (1x)

**Programlama yazılımı AS284-NETW (kilit ayarları)**

* Teslimat kapsamı: Ağ uygulamaları için kilitleri yapılandırmak ve parametreleri ayarlamak için USB bağlantı kablosu

**Sunucu Yönetim Yazılımı AS 274**

* 100'den fazla kilit ve kullanıcıyı yönetin
* Bulundurur: 1 APHI Ethernet RJ45

**Aksesuarlar**

**AS284-OW Operatörü**

* AS284-USBW ve AS284-NETW programlama yazılımı için USB

**AS284-AW Yöneticisi**

* AS284-NETW programlama yazılımı için USB

**İşlevsellik**

**Kod İşlevleri**

* Yakın kod ile bir defa kombinasyon, dahili; pil durumu ve kilit / kapı etkinliği geri bildirimi
* Geçici kod geçerliliği
* Değiştirilebilir mod (bir defalık ve/veya banka modu)
* 4 yanlış koddan sonra yanlış kilitleme özelliği
* Zorlama kodu (sessiz alarm)
* Tekli mod (1 x 6 hane)
* Çift mod (2 x 6 hane)
* Raf işlevi

**Zaman Kilidi İşlevleri**

* Zaman gecikmesi
* Zorlama zamanı gecikmesi
* Açılış penceresi
* Zaman kilidi süreleri (banka modu)
* Geri dönüşsüz gecikme
* Otomatik DLST (yaz / kış saati) değişimi

**Uygulamalar**

**AS284-NETW Programlama Yazılımı**

* Axessor USB (yalnızca bağımsız), Axessor IP ve Axessor CIT gibi Axessor Serisi ürünlerini yapılandırmak ve parametreleri ayarlamak için AS284-NETW yazılımını kullanın.
* Axessor IP veya Axessor CIT sistemlerinde AS284-NETW uzaktan yönetim veya genel olarak ağa bağlı işletim (eBox kullanarak) için kullanılabilir.

**Önceki sürümde yapılan değişiklikler:**

**AS284-W sürüm 4.0.0.63**

* Sanal ortamlarda birden fazla AS284-W örneği desteği

**AS284-W sürüm 4.0.0.61**

* 4.0 yerine .Net 4.5 tabanlı
* Denetim görüntüleyici donanım kilidi için hazırlık
* SDK dongle'larına hazırlık
* Birkaç hata düzeltmesi

**AS284-USBW Programlama Yazılımı**

Axessor USB, Axessor IP ve Axessor CIT gibi Axessor Serisi ürünlerini yapılandırmak ve parametreleri ayarlamak için AS284-USBW yazılımını kullanın.

Bu yazılım yalnızca bağımsız kullanım amaçlıdır (ağ işlevselliği yoktur).

**Önceki sürümde yapılan değişiklikler:**

**AS284-W sürüm 4.0.0.63**

* Sanallaştırılmış ortamlarda birden fazla AS284-W örneği desteği

**AS284-W sürüm 4.0.0.61**

* 4.0 yerine .Net 4.5 tabanlı
* Denetim görüntüleyici donanım kilidi için hazırlık
* SDK dongle'larına hazırlık
* Birkaç hata düzeltmesi

**AS280-INSW Kurulum / Etkinleştirme Yazılımı**

Ağ kilitlerini (eBox ile Axessor IP / CIT) kurmak ve bir defalık kombinasyon modunu (yalnızca Axessor CIT) etkinleştirmek için AS280-INSW yazılımını kullanın.

Bu yazılımı indirmek için dormakaba SafeLocks'a kayıtlı olmanız gerekmektedir. Lütfen dormakaba SafeLocks Support sl-techsupport.ch@kaba.com ile iletişime geçin.